
In hamvoip

pacman -S alsa-lib alsa-utils

pacman -S lsb-release







Type alsamixer




Select the auto gain control



Press “**M**” to disable



Then press tab until it shows like this below:-



Then use <- , -> to select mic and PCM to adjust according to your level of audio input/output, test it with your Handly to echolink, and vice versa to get your optimized end results (sweatspot)

ESC will save your setting